Maintenance Guide

**Mat Cleaning Guidelines**

For best results, tiles should be cleaned regularly. Simply follow these instructions to keep your tile looking great and functioning effectively.

**PVC Non coated Turtle Tiles**

Sweep regularly, dry or wet mop the surface. Tiles can be lifted if you desire to clean the floor under them. Wet mop with mild soap or detergent. For best results, use a detergent with a pH between 4 and 9.

**Entrance tiles (with carpet inlays)**

Sweep or vacuum regularly, Tiles can be lifted if you desire to clean the floor under them. Carpet may be shampooed with a mild soap or detergent. For best results, use a detergent with a pH between 4 and 9.

**pvc coated turtle tiles:**

**Dura coat**

DURA CRIB AND DURA STAT CLEANING GUIDELINES