

**2022 Lift Bag Protection & Pad Kits** 7400 Industrial Parkway Drive Lorain, OH 44053 (800) 756-6635 orders@turtleplastics.com

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Photo | Kit Name | Mod Pad Lifting Kit A Small | Mod Pad Lifting Kit B Small | Mod Pad Lifting Kit C Small | Mod Pad Lifting Kit 10Medium | Mod Pad Lifting Kit 28Medium | Mod Pad Lifting Kit10MTop Bag Pad |
|  |  |  | Part # | Part # | Part # | Part # | Part # | Part # |
|  | Component | Description | MPLK | MPLK | MPLK | MPLK | MPLK | MPLK |
|  | A | B | C | 10M | 28M | 10MTBP |
| A picture containing text  Description automatically generated | CTP1818- 1.5 | 18"x18"x11/2"Mod Pad® w/Level | 2 | 2 | 2 |  |  |  |
| A picture containing text  Description automatically generated | 44PL-18 | 4”x4”x18”Hybrid Crib® | 3 | 18 | 27 |  |  |  |
| A picture containing sky, outdoor  Description automatically generated | 4/4-20 | 4”x4”x20”Wedge | 2 | 2 | 2 |  |  |  |
| A picture containing text, case  Description automatically generated | CTP2424-2W/L | 24"x24"x2"Mod Pad®w/Level |  |  |  | 2 | 2 | 2 |
|  | 67SC-24 | 6”x7”x24”Super Crib® |  |  |  | 3 | 12 | 6 |
|  | 6/7-24 | 6”x7”x24”Super Wedge |  |  |  | 2 | 2 | 2 |
| A picture containing text  Description automatically generated | TBP | Top Bag Pad |  |  |  |  |  | 1 |
|  | Weight (in lbs.) | 59 | 149 | 203 | 162 | 391 | 250 |
|  |

\*\*\*Are you conducting Fleet Maintenance? Please call us to inquire about our new Fleet Maintenance Starter Kit
that includes many of our most popular components with additional industrial cribbing to help stabilize

heavy equipment and/or apparatus during repairs. Reference Part #FMBS.